* 1 end effector and mount
* 1 z-probe tower
* 1 Alex extruder
* 1 power supply mount (set)
* 3 motor frames
* 3 top frames
* 3 FSR glass tabs
* 3 carriages
* 3 carriage rail
* 3 sliders
* 3 end stops mounts
* 1 end effector
* 1 z-probe tower
* 1 extruder (airtripper designed for geared stepper)
* 1 power supply mount (set)
* 3 motor frames
* 3 top frames
* 3 glass tabs and spiral hold downs
* 3 carriage adapters (optional)
* 3 carriages
* 6 end stops mounts
* 1 JHead mount
* 1 Fan mount